---
title: pymc-repeater KISS TNC Re-enumeration Fix
type: runbook
tags:
  - mesh
aliases: []
related:
  - [[recon-operations]]
  - [[SESSION-HANDOFF-meshai-test]]
  - [[meshtasticd-sim-nodes-runbook]]
  - [[meshtastic-headscale-runbook]]
  - [[syncthing-add-node]]
updated: 2026-07-13
---
# pymc-repeater KISS TNC Re-enumeration Fix

`pymc-repeater.service` on **aida-nebra** (Tailscale 100.64.0.9) runs the Meshcore LoRa repeater node `EchoBase` on 910.525 MHz SF7. It talks to a RAK4631 USB KISS TNC (VID 239a / PID 8029) via the `/dev/pymc-radio` udev symlink. The Nebra SX1262 hat on the same machine runs a separate `meshtasticd` instance on its own radio — see [[meshtastic-sidecar-node]] for that hardware's setup. Do not touch `meshtasticd` or the SX1262 hat during any pymc-repeater work.

---

## Background — Why This Breaks

`KissModemWrapper` holds the serial file descriptor open but has no reopen logic. When the RAK4631 re-enumerates (power cycle, USB glitch, kernel rescan), the kernel assigns a new node: observed `ttyACM0` → `ttyACM1` around 2026-06-23. The service keeps a stale fd pointing at `/dev/ttyACMx (deleted)`. Systemd still reports `active (running)` — the service is silently deaf and mute.

---

## Symptom

Every ~30 seconds in the journal:

```
KissModemWrapper - ERROR - Serial write error: ... [Errno 5] Input/output error
TX frame write failed, dropping frame
```

Zero RF traffic in or out despite a green `systemctl status`.

---

## Diagnose

### 1. Check the journal for the I/O error spam

```bash
ssh zvx@100.64.0.9
journalctl -u pymc-repeater.service --since '5 min ago' --no-pager
```

Look for `[Errno 5] Input/output error` or `TX frame write failed` — either confirms stale fd.

### 2. Inspect the process's open file descriptors

```bash
sudo ls -l /proc/$(systemctl show -p MainPID --value pymc-repeater.service)/fd/ | grep ttyACM
```

- **Stale (broken):** symlink target contains `(deleted)` — smoking gun.
- **Healthy:** target points at a real `/dev/ttyACMx`.

### 3. Confirm where the device landed after re-enumeration

```bash
ls -l /dev/pymc-radio
```

Shows which `ttyACM*` the live RAK4631 is on now.

---

## Manual Recovery

A restart clears the stale fd and re-opens the device via the udev symlink:

```bash
sudo systemctl restart pymc-repeater.service
```

### Verify recovery

```bash
# fd should now point at a real ttyACMx (not deleted)
sudo ls -l /proc/$(systemctl show -p MainPID --value pymc-repeater.service)/fd/ | grep ttyACM

# Journal should show reconnect and normal TX
journalctl -u pymc-repeater.service -n 20 --no-pager
```

Expected healthy journal lines:

```
KISS modem connected to /dev/pymc-radio at 115200 baud
Retransmitted packet ...
```

The `[Errno 5]` spam must be absent.

---

## Permanent Fix (applied 2026-07-01)

Two changes make pymc-repeater self-healing across any future re-enumeration. Original files were backed up as `.bak` alongside each.

### 1. udev rule — `/etc/udev/rules.d/99-pymc-radio.rules`

Added `TAG+="systemd"` and `ENV{SYSTEMD_WANTS}="pymc-repeater.service"` to the existing VID 239a / PID 8029 rule:

```udev
SUBSYSTEM=="tty", ATTRS{idVendor}=="239a", ATTRS{idProduct}=="8029", \
  SYMLINK+="pymc-radio", \
  TAG+="systemd", \
  ENV{SYSTEMD_WANTS}="pymc-repeater.service"
```

On any future re-enumeration, udev creates the `dev-pymc\x2dradio.device` unit for the new node and systemd activates `pymc-repeater.service` against it automatically.

### 2. systemd unit — `/etc/systemd/system/pymc-repeater.service`

`[Unit]` additions:

```ini
BindsTo=dev-pymc\x2dradio.device
After=dev-pymc\x2dradio.device
StartLimitIntervalSec=300
StartLimitBurst=10
```

`[Service]` additions:

```ini
Restart=always
RestartSec=5
```

`BindsTo` stops the service cleanly when the TNC drops (the device unit disappears) and restarts it when the device returns. `Restart=always` with `RestartSec=5` ensures fast recovery from any modem crash without the device unit cycling.

---

## Verify the Resilience Wiring Is Intact

Run these on aida-nebra after any future maintenance to confirm the permanent fix is still in place:

```bash
# BindsTo and After wired to the device unit
systemctl show pymc-repeater.service -p BindsTo -p After | grep -i pymc

# udev tagging correct
udevadm info -q property -n /dev/pymc-radio | grep -i SYSTEMD

# device unit tracked by systemd
systemctl list-units --type=device --all | grep -i pymc
```

Expected output:

```
BindsTo=dev-pymc\x2dradio.device
After=... dev-pymc\x2dradio.device ...
SYSTEMD_WANTS=pymc-repeater.service
dev-pymc\x2dradio.device  loaded active plugged  ...
```

---

## Known Secondary Issue (non-blocking)

RRD graphing fails with `rrdtool not available`. Metrics/graphing only — no impact on RF operation.

---

## Quick Reference

| Item | Value |
|------|-------|
| Host | aida-nebra (100.64.0.9) |
| Service | `pymc-repeater.service` |
| Node / freq | EchoBase, 910.525 MHz SF7 |
| TNC hardware | RAK4631 USB KISS TNC (VID 239a / PID 8029) |
| udev symlink | `/dev/pymc-radio` |
| udev rule | `/etc/udev/rules.d/99-pymc-radio.rules` |
| Unit file | `/etc/systemd/system/pymc-repeater.service` |
| Unrelated radio | Nebra SX1262 hat → `meshtasticd` (do not touch) |

```bash
# Restart (manual recovery)
sudo systemctl restart pymc-repeater.service

# Tail journal
journalctl -u pymc-repeater.service -f

# Check fd state
sudo ls -l /proc/$(systemctl show -p MainPID --value pymc-repeater.service)/fd/ | grep ttyACM
```
